INPUTS

1.100% to PC14 2.checkpoint to PA10 3.Low level to PA9 4.Water Available to PB3

LEDS

1.Checkpoint to PA10 2.Water available to PB3

SELECTION SWITCHES to PB0

MCU BOARD CONNECTIONS

RTC

SDA to PB7 SCL to PB6

RELAY to PA15

POWER SUPPLY